HUNG ESCAPEWAY LIFELINE

BELTLINE

STOPPING WITH DOOR CLOSED

FIREBOSS STATION

MINE

PHONE

AMS

AIR READING

19 FT. X 5FT.

100 FPM

BELT CHECK

COAL SPILL

48” WIDE

12” DEEP

60” LONG

TAILPIECE

FEEDER

MINE PHONE

SHUTTLE CAR 434

AIR READING 19 FT. x 5 FT.

340 FPM

HUNG LINE CURTAIN

REFLECTIVE SIGN

LAST ROW OF BOLTS

CONTINUOUS

MINER

#140

0.4% CH 4

20.8% O2

LAST ROW OF BOLTS 5 FT. FROM FACE

FACE

HUNG ESCAPEWAY LINE

HUNG UNGUARDED HIGH VOLTAGE CABLE

0.4% CH4

20.1% O2

10 LB. FIRE EXTINGUISHER

SCSR

CACHE

ENERGIZED POWER CENTER

MINER #140

BREAKER

OFF

BOLTER# 540 BREAKER

OFF

SHUTTLECAR

BREAKER OFF

SHUTTLECAR BREAKER OFF

SCOOP CHARGER # 1 BREAKER

FEEDER #3

BREAKER OFF

STOPPING WITH DOOR CLOSED

10 LB. FIRE

EXTINGUISHER

LINE CURTAIN

0.4% CH4

20.2% O2

BATTERY SCOOP ON CHARGER

NO FIRE EXTINGUISHER

SCOOP BATTERY CHARGER # 1

AIR READING

0.75FT.x1.33FT.

360FPM

STOPPING

BLOCK OUT OF STOPPING

CHECK CURTAIN

CHECK CURTAIN

SHUTTLE CAR 435

AIR READING

19 FT. X 5 FT

235 FPM

HUNG LINE CURTAIN

LAST ROW OF BOLTS 5 FT. FROM FACE

FACE

0.4% CH4

20.8% O2

REFECTIVE SIGN

“HANGING”

LAST ROW OF BOLTS

REFLECTIVE SIGN

LAST ROW OF BOLTS

TEST HOLE

60 INCHES DEEP

ROOF

BOLTER #540

0.5% CH4

20.1% O2

LAST ROW OF BOLTS 25 FT.

FROM FACE

NOT BOLTED

FACE