BELT

LINE

CAVED

CAVED

CAVED AIRTIGHT

CAVED

AIRTIGHT

4.5 % CH4

0 ppm CO

12.5% O2

BELT

LINE

UNSAFE

ROOF

UNSAFE ROOF

CAVED

CAVED

BELT LINE

4.5% CH4

0 ppm CO

12.5% O2

BARRICADE

LIVE

CONSCIOUS

“HELP GET ME OUT”

TEMPORARY

STOPPING

5.5% CH4

OppmCO

12.5% O2

BELT TAIL

CONTINUOUS

MINER

5.5% CH4

0 ppm CO

12.5% O2

FACE

# 2 ENTRY

TEMPORARY STOPPING DOOR CLOSED

5,000 CFM

BRATTICE

CLOTH

COMMAND CENTER

UNSAFE ROOF

UNSAFE ROOF

TEMPORARY STOPPING

5.5% CH4

0 ppm CO

12.5% O2

BRATTICE

CLOTH

5.5% CH4

0 ppm CO

12.0% O2

UNSAFE ROOF

UNSAFE ROOF

5.5% CH4

0 ppm CO

12.0% O2

SPLIT ENTRY AIR SHAFT INTAKE SIDE

SPLIT ENTRY AIR SHAFT 8” SOLID SEPARATION WALL

SPLIT ENTRY AIR SHAFT 8” SOLID SEPARATION WALL

SPLIT AIR SHAFT RETURN SIDE

5.5% CH4

0 ppm CO

12.5% O2

BRATTICE CLOTH

5.5% CH4

0ppm CO

12.5% O2

BODY

R/A

DOOR OPEN

DOOR OPEN

LINE

CURTAIN

BATTERY PHONE

SHUTTLE CAR

5.5% CH4

0ppm CO

12.0% O2

5.5% CH4

0ppm CO

12.0% O2

BRATTICE CLOTH

BRATTICE CLOTH

FACE

# 3 ENTRY

TEMPORARY STOPPING

UNSAFE ROOF

UNSAFE ROOF

START OF SMOKE

END OF SMOKE

START OF SMOKE



SCOOP ON FIRE

BRATTICE CLOTH

START OF SMOKE



START OF SMOKE



UNSAFE ROOF

UNSAFE ROOF

5.5% CH4

O ppm CO

12.5% O2

BARRICADE

BODY

ROOF BOLTER

FACE