FACE

BODY

COMMAND CENTER AND CLOCK

LINE CURTAIN

CAVED

CAVED

PERMANENTSTOPPING DOWN

BRATTICE CLOTH

OVERCAST WALL

4 % CH4

5 ppm CO

18 % O2

BARRICADE

BODY

ROOF BOLTER

FACE

#2 ENTRY

DOOR ON SURFACE FOR ELEVATOR IS OPEN

RETURN SIDE OF AIR SHAFT

SEPERATION WALL OF SHAFT FROM THE SURFACE TO MINE FLOOR

SEPERATION WALL OF SHAFT FROM THE SURFACE TO MINE FLOOR

INTAKE SIDE OF AIR SHAFT WITH ELEVATOR IN SHAFT

ELEVATOR DOOR OPENS WHEN ON THE BOTTOM OF SHAFT

PUMP POWER CABLE FROM SURFACE

PUMP BREAKER

BATTERY PHONE

PERMANENT STOPPING

BRATTICE CLOTH

OVERCAST WALL

OVERCAST WALL DOOR OPEN

OVERCAST WALL

6 TIMBERS

UNSAFE ROOF

UNSAFE ROOF

BRATTICE CLOTH

WATER ROOFED

WATER ROOFED

5 % CH4

5 ppm CO

18 % O2

RAM CAR

CONTINUOUS MINER

FACE

#3 ENTRY

FACE

BRATTICE CLOTH

BRATTICE CLOTH

PUMP CABLE

STATIONARY PUMP

WATER ROOF

WATER ROOFED

UNCONSCIOUS LIVE PERSON

5 % CH4

5 ppm CO

18 % O2

CAVED

UNSAFE ROOF

PERSON

BODY

OPEN BOREHOLE

4 %CH4

200 ppm CO

18.0% O2

TEMPORARY

STOPPING DOWM

BATTERY SCOOP ON FIRE

CAVED

CAVED

BATTERY MAN-TRIP

BOTTOM OF SLOPE

5 % CH4 5ppm CO

18 % O2

BARRICADE

LIVE MAN TALKING

“HELP GET ME OUT”

CAVED

CAVED

TOP OF SLOPE

TOP OF SLOPE TO CAVED AREA EXPLORED BY PREVIOUS TEAM