**# 1 entry & X-cuts to # 2 entry**

**POST 5 MINE RESCUE DAY # 2**

**CAVED AIRTIGHT**

**EXHAUST FAN**

**EXHAUST FAN SWITCH OFF**

**B/O – CCA ON SURFACE**

**BRATTICE CLOTH**

**No. 1 PUMP SWITCH OFF**

**PUMP CABLE**

**5.5% CH4**

**10 PPM CO**

**19.2% O2**

**UNSAFE ROOF**

**UNSAFE ROOF**

**CONSCIOUS**

**(“HELP THE ROOF IS UNSAFE ON BOTH SIDES OF ME”)**

**SUMP**

**BATTERY**

**MINE PHONE**

**UNSAFE ROOF**

**UNSAFE ROOF**

**PERMANENT STOPPING DOWN**

**5.5% CH4**

**10 PPM CO**

**19.5% O2**

**LINE CURTAIN**

**1.5% CH4**

**8 PPM CO**

**19.5% O2**

**TEMPORARY STOPPING DOWN**

**5.5% CH4**

**10 PPM CO**

**18.5% O2**

**WATER OVER KNEE DEEP**

**WATER OVER KNEE DEEP**

**BRATTICE CLOTH**

**8 TIMBERS**

**BODY**

**No. 1 STATIONARY PUMP WITH DISCHARGE LINE TO SURFACE**

**WATER ROOFED**

**USED SCSR**

**5.5% CH4**

**10 PPM CO**

**19.2% O2**

**BARRICADE**

**LUNCH PAIL**

**USED SCSR**

**BRATTICE CLOTH**

**FACE**

**# 2 ENTRY & X-CUTS TOWARD # 3**

**CAVED AIRTIGHT**

**CAVED**

**BRATTICE CLOTH**

**BATTERY SCOOP**

**5.5% CH4**

**10 PPM CO**

**19.5% O2**

**WATER OVER KNEE DEEP**

**PERMANENT STOPPING DOWN**

**CAVED**

**TEMPORARY STOPPING DOWN**

**BRATTICE CLOTH**

**UNSAFE RIB**

**COAL HAULER**

**4.0% CH4**

**10 PPM CO**

**19.2% O2**

**BARRICADE**

**4.0% CH4**

**51 PPM CO**

**19.5% O2**

**CONSCIOUS**

**(“HELP GET ME OUT OF HERE”)**

**4.0% CH4**

**51 PPM CO**

**19.5% O2**

**WATER OVER KNEE DEEP**

**WATER OVER KNEE DEEP**

**WATER OVER KNEE DEEP**

**WATER OVER KNEE DEEP**

**START OF SMOKE**

**END OF SMOKE**

**BARRICADE**

**BLOWN DOWN**

**CONTINUOUS MINER ON FIRE**

**REMOTE BOX**

**FACE**

**# 3 ENTRY**

**5.5% CH4**

**10 PPM CO**

**19.5% O2**

**CAVED**

**FLAGGING**

**TAPE**

**5.5% CH4**

**10 PPM CO**

**19.4% O2**

**1.5% CH4**

**8 PPM CO**

**19.5% O2**

**WATER KNEE DEEP**

**4.0% CH4**

**9 PPM CO**

**19.1% O2**

**WATER KNEE DEEP**

**BRATTICE CLOTH**

**AIR SHAFT**

**FACE**