**# 1 entry and cross cuts to the right**

**4% CH4**

**0 PPM CO**

**19.5% 02**

**CAVED**

**CAVED**

**TEMPORARY STOPPING DOWN**

**LINE CURTAIN**

**WATER OVER KNEE DEEP**

**WATER**

**ANKLE**

**DEEP**

**BRATTICE CLOTH**

**BODY**

**6% CH4**

**0PPM CO**

**13% O2**

**CAVED**

**# 2 ENTRY & CROSS CUTS TO # 3**

**CAVED AIRTIGHT**

**BOREHOLE TO SURFACE**

**PUMP POWER SWITCH**

**ON/OFF**

**FREASH AIR BASE CLOCK & DATE BOARD**

**PUMP POWER CABLE AND DISCHARGE LINE**

**BATTERY SCOOP**

**TEMPORARY STOPPING DOWN**

**6% CH4**

**0 PPM CP**

**12% O2**

**END OF 10 FT. OF SUCTION LINE**

**STATIONARY PUMP WITH DISCHARGE LINE AND POWER CABLE TO SURFACE**

**6% CH4**

**O PPM CO**

**13 % O2**

**WATER OVER KNEE DEEP**

**WATER ANKLE**

**DEEP**

**WATER OVER KNEE DEEP**

**WATER ANKLE**

**DEEP**

**BRATTICE CLOTH**

**BATTERY SCOOP**

**6 % CH4**

**0 PPM CO**

**12 % O2**

**6% CH4**

**0 PPM CO**

**13 % 02**

**BARRICADE**

**LIVE CONSCIOUS MAN**

**“HELP, IT IS AIRTIGHT BEHIND” ME”**

**FACE**

**# 3 ENTRY**

**CAVED AIRTIGHT**

**CAVED AIRTIGHT**

**CAVED**

**EXHAUST FAN AIR SHAFT**