JA Problem No. 1 Correction

Add a brattice cloth to the FAB when working this problem.

A stopping was left out unintentionally when designed and it will be needed to cause all the air to clear explosive mix off the pump cable in Ventilation 1.

Also, there may be other ways to vent this problem correctly