FEDERAL #14 MINE

VENTILATION PLAN

* Line curtains are required to be installed to within 5’ of the face or to the next to last complete row of permanent support.
* 7000CFM of air is required when coal is being mined, cut, or loaded.
* 15,000 CFM is required in the last open crosscut on the working section at all times.
* The face of any entry shall not be driven more than 40’ inby the proposed crosscut off that entry.
* During the bolting cycle the line curtain shall be maintained to within 10’ from the bumper of the bolter with a minimum of 3,000 CFM at the inby end of the line curtain.