1.

ENERGIZED

2.

4” FRESH

WATER LINE

4” SHUT OFF

3.

VALVE IN OFF

POSITION

B/O STATION

4.

&

CLOCK

FIRE

5.

HOSE

6.

BRATTICE

CLOTH

7.

TEMPORARY

STOPPING

START OFF

8.

SMOKE

END OF

SMOKE

4 % CH4

9.

250 PPM CO

18 % O2

UNDERCAST

10.

4 % CH4

11.

250 PPM CO

18 % O2

FIRE NOZZLE TURNED OFF

12.

13.

CAVED

AIRTIGHT

14.

CAVED

AIRTIGHT

15.

START OFF

16.

SMOKE

END OF

SMOKE

17.

UNSAFE

ROOF

18.

UNDERCAST

WALL

19.

LIVE

UNCONSCIOUS

20.

UNSAFE

ROOF

21.

UNDRCAST

WALL

22.

UNSAFE

ROOF

23.

BODY

24.

SCOOP

ON FIRE

25.

R/A

START OFF

26.

SMOKE

END OF

SMOKE

27.

DOOR

OPEN

PURGE

28.

VALVE

CLOSED

29.

DOOR

CLOSED

30.

LIVE

UNCONSCIOUS

31.

CAVED

AIRTIGHT

32.

CAVED

AIRTIGHT

33.

START OFF

34.

SMOKE

END OF

SMOKE

35.

UNSAFE ROOF