The EPDM breathing hoses use .

1. Quarter turn connectors
2. Bayonet Rings
3. Nothing

The factory cartridge is good for 4 years from the manufacture date.

1. Filled
2. Packed
3. Stored

The weight of a fully charged BG-4 apparatus is 15kg ( lbs)

1. 32
2. 33
3. 34

To start the alarm, press the Yellow panic button in center of the Sentinel.

1. Manuel
2. Main
3. Loud

The valve opens at more than 10 mbar.

1. Drain
2. Drainage
3. Relief

The venting hole located in the must point upwards.

1. Air cooler
2. Cover for cooler
3. Lid

A minimum of 2600 psi is needed for a to perform a proper high pressure leak test.

1. Sentinel
2. Monitron
3. Neither A or B

Do not re-use cartridges.

1. Sweatshop
2. Factory
3. used