1. Lubricating oil and grease kept underground shall be stored in fireproof,

closed metal containers.

a. used b. stored c. kept

2. All fire suppression devices shall be visually inspected at least once each

week by a person qualified to make such inspections.

a. suppression b. fighting c. containment

3. Chemical extinguishers shall be examined every 6 months and the date of the

examination shall be written on a permanent tag attached to the extinguisher.

a. tested; test b. examined; examination c. checked; check

4. The operator must maintain a 300 foot diameter barrier around oil and gas

wells, unless a lesser barrier consistent with State laws and regulations is

approved.

a. 300 b. 500 c. 1000

5. The mine emergency evacuation and firefighting program is required to

instruct all miners in the use, care and maintenance of self-rescue devices.

a. escape b. training c. firefighting

6. The mine emergency evacuation and firefighting program requires a review

of the mine map, the escapeway system, and location of refuge alternatives.

a. escape b. training c. firefighting

7. Track haulage roads should have a continuous clearance on one side of at

least 24 inches from the farthest projection of normal traffic.

a. protrusion b. projection c. overhang

8. Welding, cutting and soldering with an arc or flame are prohibited within 150

feet of a seal.

a. 150 b. 300 c. 500

9. A bar for taking down loose material shall be available in the working place

or on all face equipment except haulage equipment.

a. belt feeders b. diesel equipment c. haulage equipment

10. Methane is lighter than air.

 a. Hydrogen b. Methane c. Nitrogen

1. c

2. a

3. b

4. a

5. c

6. c

7. b

8. a

9. c

10. b

1. Lubricating oil and grease \_\_\_\_\_\_ underground shall be stored in fireproof,

closed metal containers.

a. used b. stored c. kept

2. All fire \_\_\_\_\_\_\_\_ devices shall be visually inspected at least once each

week by a person qualified to make such inspections.

a. suppression b. fighting c. containment

3. Chemical extinguishers shall be \_\_\_\_\_\_\_\_ every 6 months and the date of the

examination shall be written on a permanent tag attached to the extinguisher.

a. tested; test b. examined; examination c. checked; check

4. The operator must maintain a \_\_\_\_\_\_\_ foot diameter barrier around oil and gas

wells, unless a lesser barrier consistent with State laws and regulations is

approved.

a. 300 b. 500 c. 1000

5. The mine emergency evacuation and \_\_\_\_\_\_\_\_\_\_\_ program is required to

instruct all miners in the use, care and maintenance of self-rescue devices.

a. escape b. training c. firefighting

6. The mine emergency evacuation and \_\_\_\_\_\_\_\_\_\_ program requires a review

of the mine map, the escapeway system, and location of refuge alternatives.

a. escape b. training c. firefighting

7. Track haulage roads should have a continuous clearance on one side of at

least 24 inches from the farthest \_\_\_\_\_\_\_\_\_\_\_\_\_\_ of normal traffic.

a. protrusion b. projection c. overhang

8. Welding, cutting and soldering with an arc or flame are prohibited within \_\_\_\_\_\_\_\_\_

feet of a seal.

a. 150 b. 300 c. 500

9. A bar for taking down loose material shall be available in the working place

or on all face equipment except \_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_.

a. belt feeders b. diesel equipment c. haulage equipment

10. \_\_\_\_\_\_\_\_\_\_\_ is lighter than air.

 a. Hydrogen b. Methane c. Nitrogen