**# 1 entry and x-cuts toward # 2 entry**

**COMMAND CENTER FOR B/O & CCA**

**PUMP SWITCH ON/OFF FAN SWITCH ON/OFF**

**DATE BOARD & CLOCK**

**TOP OF SLOPE**

**BATTERY PAGER PHONE**

**BOTTOM OF**

 **SLOPE**

**5 % CH4**

**10 PPM CO**

**19 % O2**

**4 % CH4**

**10 PPM CO**

**19 % O2**

**TEMPORARY STOPPING DOWN**

**DISABLED**

**BATTERY MANTRIP**

**UNSAFE ROOF**

**UNSAFE ROOF**

**TEMPORARY STOPPING DOWN**

**DE-ENERGIZED**

**POWER CENTER**

**RADIO WITHOUT A BATTERY**

**BATTERY FOR A RADIO**

**CAVED AIRTIGHT**

**CAVED AIRTIGHT**

**FACE**

**# 2 ENTRY AND X-CUTS TO 3**

**PUMP CABLE IN POWER BOREHOLE TO THE SURFACE**

**PERMANENT STOPPING DOOR OPEN**

**WATER ANKLE DEEP**

**25 FT. OF PUMP POWER CABLE**

**WATER KNEE DEEP**

**PUMP**

**5 % CH4**

**10 PPM CO**

**19 % O2**

**SUCTION LINE**

**WATER ROOFED**

**BRATTICE CLOTH**

**5 % CH4**

**10 PPM CO**

**19 % O2**

**UNSAFE ROOF**

**4 % CH4**

**10 PPM CO**

**19 % O2**

**TEMPORARY STOPPING**

**LIVE PERSON**

**“HELP”**

**BATTERY PHONE**

**3 TIMBERS**

**5 % CH4**

**10 PPM CO**

**19 % O2**

**BRATTICE CLOTH**

**UNSAFE RIB**

**5 % CH4**

**10 PPM CO**

**19 % O2**

**BRATTICE CLOTH**

**DIESEL RAM CAR**

**BRATTICE CLOTH**

**BRATTICE CLOTH**

**5 % CH4**

**10 PPM CO**

**19 % O2**

**CONTINUOUS**

**MINER**

**LINE CURTAIN**

**CAVED**

**FACE**

**# 3 ENTRY**

**8 FT. DIA. AIR SHAFT**

**BODY**

**WATER ROOFED**

**5 % CH4**

**10 PPM CO**

**19 % O2**

**WATER KNEE DEEP**

**WATER ANKLE DEEP**

**OPEN BOREHOLE**

**BRATTICE CLOTH**

**5 % CH4**

**10 PPM CO**

**19 % O2**

**CAVED**

**CAVED**

**5 % CH4**

**10 PPM CO**

**19 % O2**

**4 % CH4**

**10 PPM CO**

**10 % O2**

**BARRICADE**

**LIVE CONSCIOUS**

**MAN**

**“HELP ME I HAVE AN AIRTIGHT FACE BEHIND ME.”**

**FACE**