4.5 % CH4

0 PPM CO

18.1 % O2

BARRICADE

TWO TIMBERS

LIVE PERSON

CONSCIOUS

TALKING

WATER

KNEE DEEP

LINE CURTAIN

RETURN SIDE OF SHAFT WITH HOIST

DATE BOARD

DIVIDER WALL

INTAKE SIDE

OF SHAFT

5.9 % CH4

0 PPP CO

19.0 % O2

5.8 % CH4

0 PPM CO

18.2 % O2

UNSAFE RIB

3.9 % CH4

3 PPM CO

19.5 % O2

CUT INTO

OLD WORKS

2 TIMBERS

5.1 % CH4

0 PPM CO

19.8 % O2

BAGS OF

ROCK DUST

BOLT

MACHINE

CAVED

AIRTIGHT

WATER

KNEE DEEP

UNSAFE ROOF

UNSAFE ROOF

WATER

ROOFED

WATER

KNEE DEEP

SATAIONARY

ELECTRIC

SUMP PUMP

PUMP CABLE

OVERCAST

WALL WITH

DOOR OPEN

DOOR

CLOSED

OVERCAST

WALL

BOREHOLE

WITH PUMP

CABLE TO SURFACE

5.1 % CH4

2 PPM CO

19.3 % O2

BATTERY

SCOOP

OVERCAST

WALL WITH

DOOR OPEN

DOOR

CLOSED

OVERCAST

WALL WITH

DOOR OPEN

DOOR

CLOSED

5.7 % CH4

0 PPM CO

19.9 % O2

2.7 % CH4

0 PPM CO

18.6 % O2

CAVED

CAVED

2 TIMBERS

CONTINUOUS

CUTTER

FACE

UNSAFE

ROOF

UNSAFE

ROOF

PERSON

BODY

SMALL

FIRE

UNSAFE RIB

UNSAFE RIB

5.3 % CH4

0 PPM CO

18.9 % O2

BARRICADE

UNCONSCIOUS

LIVE PERSON

CAVED

FACE