BOREHOLE

FROM SURFACE

WITH ELECTRIC PUMP CABLE AND DISCHARGE LINE

5.2 % CH4

0 PPM CO

19.3 % O2

PUMP CABLE

AND

DISCHARGE

LINE

BARRICADE

CONSCIOUS

LIVE PERSON

TALKING

5.3 % CH4

2 PPM CO

19.4 % O2

STATIONARY

ELECTRIC

PUMP

WATER

ROOFED

BODY

CAVED

PERMANENT

STOPPING

INTACT

OVERCAST

WALL WITH

DOOR CLOSED

BRATTICE

CLOTH

UNSAFE

ROOF

BARRICADE

BODY

UNSAFE

RIB

UNCONSCIOUS

LIVE

PERSON

BATTERY

MINE

PHONE

3

TIMBERS

CONTINUOUS

MINER

4.9 % CH4

7 PPM CO

19.4 % O2

BARRICADE

LINE

CURTAIN

5.2 % CH4

11 PPM CO

19.1 % O2

UNSAFE

ROOF

LUNCH

PAIL

BODY

CUT INTO

OLD WORKS

CAVED

AIRTIGHT

BATTERY

MANTRIP

TEMPORARY

STOPPING

INTACT

SCOOP

CHARGER

WATER

ROOFED

WATER

ROOFED

BODY

BATTERY

SCOOP

5.1 % CH4

4 PPM CO

19.4 % O2

OVERCAST

WALL

UNSAFE

ROOF

UNSAFE

ROOF

PERSON

UNCONSCIOUS

LIVE

PERSON

UNSAFE

ROOF

UNSAFE

ROOF

BATTERY

MINE

PHONE

END

OF

SMOKE

SMOKE

END

OF

SMOKE

SMOKE

3

TIMBERS

FACE

TEMPORARY

STOPPING

INTACT

SHUTTLE

CAR

LOADED

5.4 % CH4

3 PPM CO

19.6 % O2

BRATTICE

CLOTH

CAVED

CAVED

AIR

SHAFT

FACE

BRIEFING

OFFICER