1. Three \_\_\_\_\_\_\_\_ socket head screws are used in the battery cover of the Sentinel.
2. octagon
3. hexagon
4. square
5. Rubber parts must be particularly protected from direct exposure to \_\_\_\_\_\_\_\_\_\_.
6. radiation
7. sunlight
8. heat
9. Disinfect parts by \_\_\_\_\_\_\_\_\_ them in a disinfectant bath using an approved disinfectant.
10. spraying
11. wiping
12. immersing
13. CO2 absorber is \_\_\_\_\_\_\_\_ approved for use after indicated expiration date.
14. possibly
15. not
16. sometimes
17. U.S. Department of Transportation requires hydro tests on composite cylinders every \_\_\_\_ years.
18. 5
19. 4
20. 10
21. The pressure reducer should be replaced after at least \_\_\_\_ years usage.
22. 5
23. 10
24. 6
25. The BG-4 is approved for use at temperatures above \_\_\_ degree C (\_\_\_ degree F)
26. -10, 32
27. 0, 28
28. -5, 23
29. Only oxygen (\_\_\_\_\_\_\_ grade or \_\_\_\_\_\_\_\_\_) with > 99.5% purity is to be used to fill the BG-4 oxygen cylinders.
30. medical, better
31. medical, equivalent
32. medical, compressed
33. Pressurized \_\_\_\_\_\_\_\_\_ in contact with oil, grease, or other contamination can result in fire or explosion.
34. air
35. components
36. oxygen
37. A defective pressure reducer is the probable cause if the manual \_\_\_\_\_\_\_\_ valve does not blow-off.
38. minimum
39. by-pass
40. drain