Use Indelible Pencil or Ink PRESHIFT - CERTIFIED EXAMINER’S REPORT Report Shall Be Signed When Finished

Date of Examination \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Time from: \_\_\_\_\_\_\_\_\_\_\_ AM/PM To: \_\_\_\_\_\_\_\_\_\_\_\_\_ AM/PM

Section/Area Reported Outside? Yes \_\_\_\_\_ No \_\_\_\_ Time: \_\_\_\_\_\_\_\_ AM/PM

Reported By: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Received By: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ INITIAL) (AUTHORIZED PERSON)

**Preshift required within 3 hours prior to any 8-hour interval.**

|  |  |  |
| --- | --- | --- |
| **Location** | **Hazardous condition** | **Action taken** |
| **Power Center** | **480 volt pump not labeled** | **Danger off or labeled to identify** |
| **Power Center** | **480 volt pump not labeled** | **Danger off or labeled to identify** |
| **No. 1 entry face** | **Cut at face 25 feet deep** | **Hazard card** |
| **No. 1 entry face** | **Cut at face not bolter w/in 24 hrs** | **Hazard card** |
| **1 to 2 entry, xc 35** | **Check curtain down** | **Re-hung** |
| **1 to 2 entry xc 37** | **Missing fire ext at 480 volt pump** | **Installed fire ext from PC** |
| **1 to 2 entry xc 37** | **Mandoor open** | **Closed mandoor** |
| **No. 2 entry xc 37 to 38** | **Loose bearing plate** | **Hazard card** |
| **No. 2 entry xc 37** | **Loose coal** | **Hazard card** |
| **No. 2 entry xc 36 to 37** | **Missing check curtain** | **Installed curtain** |
| No. 2 face area | **No danger flag** | **Installed danger flag** |
| No. 2 entry 2 xc35 | **Only 2 cribs in intersection** | **Hazard card** |
| **No. 2 xc35 to 36** | **Co sensor in wrong location** | **Move to center of entry** |
| **No. 3 entry face** | **19.5% O2 and 5.2 CH4** | **Knocked power** |
| **No. 3 face** | **Line curtain missing** | **hung curtain** |
| **No. 3 to 2 entry xc 35** | **Mandoor open** | **Closed mandoor** |
| **No. 3 to 2 entry xc 35** | **Sphere missing on life line** | **Hazard card** |
| **No. 3 entry xc 35 to 36** | **No fire ext.** | **Placed fire ext at location** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Air Measurements

|  |  |  |  |
| --- | --- | --- | --- |
| Location | CFM | Location | CFM |
| Last open cross cut between entry 2 and 3 | 57,996 |  |  |
|  |  |  |  |

Signed by Preshift Certified Examiner Date Certification Number

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Countersigned by Mine Foreman Date Certification Number

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_