**6.1.21 dk**

**Problem Statement**

* 4 miners missing
* Exhaust fan located off the no 3 entry
* Entries are numbered from left to right
* Previous team was blocked by roof falls in no. 1 and no. 2 entries
* An intake airshaft is located in no. 1 entry
* Mine maps are not up to date
* No. 3 entry outby the FAB is safe to ventilate through

**Written Instructions**

* Explore the entire mine
* The exhaust fan can be turned on and off from the surface command center
* BO is underground in the FAB
* Can carry only 2 brattice cloths while traveling













Problem Keys

* **Timber to battery mine phone and relocate**
* **Watch 2 crosscut rule while exploring**
* **Knowing Gas extent is important for venting this problem**
* **Make sure clear air placards are exactly where they are supposed to be**
* **One clear air placard is on the imaginary line (see gas extent map)**
* **Team not building in FAB beside overcast wall**