Statement 6.8.2021

* You are located in the FAB
* 3 miners are missing
* The exhaust fan is off
* When the fan is on, the air will come up no.3 entry and the out no. 1 entry
* BO is in crosscut between no. 2 and no. 3 entry in the FAB

Written Instructions:

* Explore the entire mine
* Carry only 2 brattice cloths while traveling
* Exhaust fan is off and cannot be reversed
* Fan can be turned on and off by command center, but never stalled during operation
* Bring all survivors to the FAB











**Problem Keys**

* Power to pump is not available until team stop 9
* Team must build at least one airlock when pumping the water roofed, even if they have explored on both sides of water roofed
* Team must vent barricade in no.2 entry before going to team stop 12
* Have all builds in place before turning off pump and turning on fan for vent 3 (water will roof in 2 minutes after pump is off)
* Team must not pass gas placard in no.3 entry inby last open crosscut ( evidence of fire behind barricade in no. 2 entry …FPA beside explosive mix gas placard